CONDOMINIUM PROPERTY WALKAROUND CHECKLIST
A practical visual review tool for Boards and Condo Managers
	PROPERTY NAME
	
	PROPERTY ADDRESS
	

	DATE
	
	COMPLETED BY
	


Use this checklist for a general visual walkaround only. It is not a building inspection, engineering assessment, Reserve Fund Study, or substitute for review by a qualified professional. Do not access roofs, attics, mechanical equipment, electrical equipment or other restricted areas unless appropriately authorized and qualified.
	#
	ITEM / WHAT TO LOOK FOR
	1
	2
	3
	N/A
	FOLLOW-UP

	A.  ROOFING & DRAINAGE

	1
	Roof covering / shingles - look for visible lifting, missing materials, deterioration or damage from accessible areas
	
	
	
	
	

	2
	Flashings - look for visible loose, damaged or displaced flashing around roof edges, vents and penetrations
	
	
	
	
	

	3
	Roof edges - look for lifting, deterioration or visible damage
	
	
	
	
	

	4
	Visible moisture concerns - note staining, sagging or other visible signs that may indicate water entry
	
	
	
	
	

	5
	Fascia - look for loose, damaged, deteriorated or missing sections
	
	
	
	
	

	6
	Soffits - look for loose, damaged, stained or missing sections
	
	
	
	
	

	7
	Eavestroughs - look for visible leaks, damage, sagging or debris buildup
	
	
	
	
	

	8
	Downspouts - confirm they appear secure and discharge away from the building where intended
	
	
	
	
	

	9
	Site drainage at building - note ponding, erosion or areas directing water toward the building
	
	
	
	
	

	B.  EXTERIOR WALL CLADDING

	1
	Wall transitions / connections - review visible transitions at roofs, foundations, windows and doors for obvious gaps or damage
	
	
	
	
	

	2
	Discolouration / streaking - note unusual staining or patterns that may warrant further review
	
	
	
	
	

	3
	Cladding condition - look for cracks, holes, dents, loose panels, warping or missing materials
	
	
	
	
	

	4
	Visible moisture damage - look for staining, rot, deterioration or other signs of water entry
	
	
	
	
	

	5
	Sealants - note visibly cracked, missing or deteriorated sealant at joints and penetrations
	
	
	
	
	

	C.  WINDOWS

	1
	Frames / sills - look for cracks, rot, warping, deterioration or damaged finishes
	
	
	
	
	

	2
	Sealant - note visible cracking, gaps, separation or missing sealant
	
	
	
	
	

	3
	Operation - where safely accessible, note windows that are difficult to open, close or secure
	
	
	
	
	

	4
	Glass - look for cracks, chips, fogging or failed sealed units
	
	
	
	
	

	5
	Flashing / drainage details - note obvious gaps, damage or staining around window openings
	
	
	
	
	


Rating: 1 = Needs Attention   |   2 = Monitor / Adequate   |   3 = Good Condition   |   N/A = Not Applicable


CONDOMINIUM PROPERTY WALKAROUND CHECKLIST - CONTINUED
	#
	ITEM / WHAT TO LOOK FOR
	1
	2
	3
	N/A
	FOLLOW-UP

	D.  EXTERIOR DOORS

	1
	Frames / thresholds - look for cracks, rot, warping, corrosion or deterioration
	
	
	
	
	

	2
	Weatherstripping / sealant - note visible gaps, missing material or deterioration
	
	
	
	
	

	3
	Operation - where safely accessible, confirm doors open, close and latch reasonably
	
	
	
	
	

	4
	Hardware / locks - note loose, damaged, corroded or non-functioning hardware
	
	
	
	
	

	5
	Glass - look for cracks, chips, fogging or damage
	
	
	
	
	

	E.  BALCONIES / PATIOS / DECKS

	1
	Surface condition - look for visible cracking, wear, deterioration, loose finishes or damage
	
	
	
	
	

	2
	Railings / guards - note visible corrosion, damage, looseness or missing components - do not load-test
	
	
	
	
	

	3
	Waterproofing / sealants - look for visible cracks, open joints, failed sealant or damaged membranes
	
	
	
	
	

	4
	Drainage - note ponding, blocked drains or obvious areas where water is not draining as intended
	
	
	
	
	

	5
	Building connections - note visible gaps, deterioration, staining or damage where the structure meets the building
	
	
	
	
	

	6
	Fascia / soffit finishes - look for loose, damaged, stained or deteriorated materials
	
	
	
	
	

	F.  FOUNDATION / BASE OF WALL

	1
	Visible cracking - note significant, widening or unusual cracks for follow-up
	
	
	
	
	

	2
	Movement / displacement - look for visible bulging, leaning, shifting or separation
	
	
	
	
	

	3
	Parging / exposed concrete - note spalling, deterioration, loose parging or exposed reinforcement
	
	
	
	
	

	4
	Drainage - note areas where grading appears to direct water toward the building
	
	
	
	
	

	G.  PARKADE

	1
	Overhead doors - note damage, corrosion or operation concerns from normal use
	
	
	
	
	

	2
	Floor / traffic surface - look for significant cracks, potholes, delamination, coating wear or damage
	
	
	
	
	

	3
	Visible leaks / staining - note active leakage, efflorescence, staining or deterioration
	
	
	
	
	

	4
	Drains - note blocked drains, ponding or obvious drainage concerns
	
	
	
	
	

	5
	Lighting - note damaged, missing or non-functioning fixtures
	
	
	
	
	

	6
	Signage / markings - note damaged, missing or difficult-to-read signage and traffic markings
	
	
	
	
	

	7
	Stairs / handrails / guards - note visible damage, looseness or deterioration - do not load-test
	
	
	
	
	

	8
	Ventilation / fire protection - note only obvious visible damage, alarms or concerns; technical systems require qualified review
	
	
	
	
	


Rating: 1 = Needs Attention   |   2 = Monitor / Adequate   |   3 = Good Condition   |   N/A = Not Applicable 

CONDOMINIUM PROPERTY WALKAROUND CHECKLIST - CONTINUED
	#
	ITEM / WHAT TO LOOK FOR
	1
	2
	3
	N/A
	FOLLOW-UP

	H.  PARKING LOT / WALKWAYS / CONCRETE

	1
	Asphalt / paved surfaces - look for potholes, significant cracking, settlement or deterioration
	
	
	
	
	

	2
	Water pooling - note recurring ponding or areas with poor drainage
	
	
	
	
	

	3
	Trip hazards - note lifted, uneven or damaged surfaces that may require attention
	
	
	
	
	

	4
	Curbs / aprons / steps / landings - look for cracking, spalling, settlement or damage
	
	
	
	
	

	5
	Exterior railings / handrails - note visible corrosion, damage or looseness - do not load-test
	
	
	
	
	

	6
	Site lighting - note leaning, damaged, missing or non-functioning fixtures
	
	
	
	
	

	7
	Catch basins / drainage - note blockages, settlement or drainage concerns
	
	
	
	
	

	I.  LANDSCAPING & SITE CONDITIONS

	1
	Retaining walls - look for leaning, cracking, movement, deterioration or drainage concerns
	
	
	
	
	

	2
	Erosion - note soil loss, washout or settlement
	
	
	
	
	

	3
	Trees / shrubs / vegetation - note overgrowth, dead material or vegetation contacting building components
	
	
	
	
	

	4
	Irrigation - note visible leaks, damaged heads or overspray against buildings where applicable
	
	
	
	
	

	5
	Drainage - note ponding, saturated areas or grading concerns
	
	
	
	
	

	J.  FENCING & GATES

	1
	Posts - look for leaning, broken, loose or deteriorated posts
	
	
	
	
	

	2
	Boards / panels - note missing, broken, loose, rotted or corroded materials
	
	
	
	
	

	3
	Gates - note sagging, damage or operation concerns
	
	
	
	
	

	4
	Hardware - look for corrosion, broken hinges, latches or missing fasteners
	
	
	
	
	

	5
	General condition - note rot, corrosion, pest damage or other visible deterioration
	
	
	
	
	

	K.  COMMON AREAS / OTHER SITE ITEMS

	1
	Interior common-area finishes - note visible damage, unusual wear, staining or water-related concerns
	
	
	
	
	

	2
	Ceilings / walls - look for staining, cracking or visible signs of water entry
	
	
	
	
	

	3
	Common-area doors - note operation, hardware or visible damage concerns
	
	
	
	
	

	4
	Garbage / recycling areas - note enclosure damage, drainage, lighting or housekeeping concerns
	
	
	
	
	

	5
	Sheds / accessory structures - note visible damage, deterioration or security concerns
	
	
	
	
	

	6
	Amenities - note visible deterioration or items requiring maintenance
	
	
	
	
	

	7
	Signage - note missing, damaged or difficult-to-read signs
	
	
	
	
	

	8
	Mechanical / service rooms - from authorized accessible areas only, note obvious leaks, unusual conditions or visible alarms; do not operate equipment
	
	
	
	
	

	9
	Fire / life-safety devices - note only obvious visible damage or missing devices; testing and technical assessment require qualified personnel
	
	
	
	
	


Rating: 1 = Needs Attention   |   2 = Monitor / Adequate   |   3 = Good Condition   |   N/A = Not Applicable 

NOTES & FOLLOW-UP ACTION LOG
Record observations, photographs, follow-up items and professional reviews that may be required.
	REF.
	OBSERVATION / LOCATION
	ACTION / FOLLOW-UP
	RESPONSIBLE
	TARGET DATE

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


Suggested follow-up categories: Routine maintenance | Contractor quotation | Condo manager follow-up | Engineering / technical review | Monitor at next walkaround
Important: Where a condition may present an immediate safety concern, restrict access as appropriate and obtain timely advice from the appropriate qualified professional. This checklist is intended to help identify items for follow-up, not to determine the technical cause, severity or required repair.
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